**DSP Lab Assignment**

**Submitted By Md. Fahim Shahriar (154440)**

**Task 1**

**Code :**

r = 0.9;

theta = pi/10;

x = [];

real = [];

img = [];

for i = -100:.5:20

x = [x i];

val = r ^ i;

real = [real val \* cos(i \* theta)];

img = [img val \* sin(i \* theta)];

end

subplot(2,1,1);

plot(x,real);

title('Real Part');

xlabel('values of n');

ylabel('x(n)');

grid on;

subplot(2,1,2);


plot(x,img);

title('Imaginary Part');

xlabel('values of n');

ylabel('x(n)');

grid on;

**Figure :**

**Task 2**

**Code :**

subplot(2,2,1);

a = 0.5;

x1 = [];

y1 = [];

for n = 0 : .5 : 10

x1 = [x1 n];

y1 = [y1 a^n];

end

plot(x1,y1);

title('0 < a < 1');

xlabel('values of n');

ylabel('x(n)');

grid on;

subplot(2,2,2);

a = 1.5;

x1 = [];

y1 = [];

for n = 0 : .5 : 10

x1 = [x1 n];

y1 = [y1 a^n];

end

plot(x1,y1);

title('a > 1');

xlabel('values of n');

ylabel('x(n)');

grid on;

subplot(2,2,3);

a = -0.5;

x1 = [];

y1 = [];

for n = 0 : .1 : 10

x1 = [x1 n];

y1 = [y1 a^n];

end

plot(x1,y1);

title('-1 < a < 0');

xlabel('values of n');

ylabel('x(n)');

grid on;

subplot(2,2,4);

a = -1.5;

x1 = [];

y1 = [];

for n = 0 : .1 : 10

x1 = [x1 n];

y1 = [y1 a^n];

end

plot(x1,y1);


title('a < -1');

xlabel('values of n');

ylabel('x(n)');

grid on;

****

**Figure :**

**Task 3**

**Code:**

A = 1.5;

Values = [0 .1 .2 .8 .9 1 1.1 1.2];

for in = 1 : 8

omega = pi \* Values(in);

x = [];

y = [];

for n = 0 : 40

x = [x n];

y = [y A \* cos(omega \* n)];

end

subplot(4,2,in);

stem(x,y);

title(['\omega = ',num2str(Values(in)) ,'\pi']);

xlabel('n');


ylabel('x(n)');


ylim([-1.5 1.5]);


yticks(-1.5:1.5:1.5);

end

**Figure :**





**Task 4**

**Figure 1:**

**Code 1:**

subplot(2,1,1);

t = 0:1/4000:2/60;

plot(t,cos(120 \* pi \* t + pi/3));

xlabel('t');

ylabel('x1(t)');

title('Analog Signal');

subplot(2,1,2);

t = 0:1/400:2/60;

stem(t,cos(120 \* pi \* t + pi/3));

xlabel('t');

ylabel('x1(t)');

title('Sampling With Frequency 400 Hz');

**Let us take two more signals and such that and . We will plot the signals and sample them with considering sampling frequency 400 Hz.**